IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2023-06-28T12:10:13"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20220517_1515(x64) - Exporter 20.2.90.12 - Alternate UI 20.2.90.12"
Application: "Autodesk Revit 2020 (ENG)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENG)"

People and organizations
  Person "erin.hay" of Organization (no name given)
  Owner history of Person "erin.hay" of Organization (no name given) | application "Autodesk Revit 2020 (ENG)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENG)" | change NOCHANGE | created 1687950519 (2023-06-28T11:08:39Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:Circle Head - Project Datum" | elevation 0.
        contains 3 elements
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:NBS_SideriseGroup_MineralWoolFireStopping_SIDERISECWFBCurtainWallFireboard 2" | object type "Compound Ceiling:NBS_SideriseGroup_MineralWoolFireStopping_SIDERISECWFBCurtainWallFireboard 2" | CEILING | names: "Compound Ceiling:NBS_SideriseGroup_MineralWoolFireStopping_SIDERISECWFBCurtainWallFireboard 2:221894" | material: layers "Compound Ceiling:NBS_SideriseGroup_MineralWoolFireStopping_SIDERISECWFBCurtainWallFireboard 2" ("NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" 25.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" | object type "Basic Wall:NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" | names: "Basic Wall:NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard:222022" | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" ("NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" 25.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" | object type "Floor:NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" | INSULATION | names: "Floor:NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard:222159" | material: layers "Floor:NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" ("NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" 25.) | property sets: IFC, COBie, BOS_General, NBS_Data

Types
  IFCCOVERINGTYPE "Compound Ceiling:NBS_SideriseGroup_MineralWoolFireStopping_SIDERISECWFBCurtainWallFireboard 2" | CEILING | 1 occurrence | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCWALLTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" | STANDARD | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" ("NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" 25.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" ("NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" 25.) | property sets: IFC, COBie, BOS_General, NBS_Data

Property sets
  IFC | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "INSULATION" (IFCTEXT)
  IFC | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    IfcExportAs = "IfcWallType" (IFCTEXT)
    IfcExportType = "INSULATION" (IFCTEXT)
  COBie | properties | on 2 objects (1 IFCCOVERING, 1 IFCWALLSTANDARDCASE)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_81_51:Mineral wool fire-stopping" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Silver" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Cavity barriers and fire stops for curtain walling and external facade applications" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "salesteam@siderise.com" (IFCTEXT)
    Material = "Mineral wool" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "n/a" (IFCTEXT)
    Name = "MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Square" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_80_81_51:Mineral wool fire-stopping" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Silver" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Cavity barriers and fire stops for curtain walling and external facade applications" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "salesteam@siderise.com" (IFCTEXT)
    Material = "Mineral wool" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "n/a" (IFCTEXT)
    Name = "MineralWoolFireStopping_SideriseCWFBCurtainWallFireboard_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Square" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCTEXT)
    Name = "Level 0" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCTEXT)
  COBie | properties | on 2 type objects
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_80_81_51:Mineral wool fire-stopping" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Silver" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Cavity barriers and fire stops for curtain walling and external facade applications" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "salesteam@siderise.com" (IFCTEXT)
    Material = "Mineral wool" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "n/a" (IFCTEXT)
    Name = "MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Square" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "www.siderise.com" (IFCTEXT)
    NBSInstanceId = "6cd07ebd-142e-4c0a-8f27-401876d13441" (IFCTEXT)
    NBSObjectId = "9df57c6d-d9db-8af2-fecd-e3041ac66c67" (IFCTEXT)
    NBSVariantId = "00000000-0000-0000-0000-000000000000" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/9df57c6d-d9db-8af2-fecd-e3041ac66c67/6cd07ebd-142e-4c0a-8f27-401876d13441" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_81_51" (IFCTEXT)
    Uniclass2015Title = "Mineral wool fire-stopping" (IFCTEXT)
    Uniclass2015Version = "Products v1.30" (IFCTEXT)
    Version = "14" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "www.siderise.com" (IFCTEXT)
    NBSInstanceId = "460389e1-c7d1-48d1-87fa-7e7108139177" (IFCTEXT)
    NBSObjectId = "9df57c6d-d9db-8af2-fecd-e3041ac66c67" (IFCTEXT)
    NBSVariantId = "00000000-0000-0000-0000-000000000000" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/9df57c6d-d9db-8af2-fecd-e3041ac66c67/460389e1-c7d1-48d1-87fa-7e7108139177" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_81_51" (IFCTEXT)
    Uniclass2015Title = "Mineral wool fire-stopping" (IFCTEXT)
    Uniclass2015Version = "Products v1.30" (IFCTEXT)
    Version = "15" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_MineralWoolFireStopping_SideriseCWFBCurtainWallFireBoard" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "www.siderise.com" (IFCTEXT)
    NBSInstanceId = "4d487aed-a085-41b4-ba65-f87f8178868d" (IFCTEXT)
    NBSObjectId = "9df57c6d-d9db-8af2-fecd-e3041ac66c67" (IFCTEXT)
    NBSVariantId = "00000000-0000-0000-0000-000000000000" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/9df57c6d-d9db-8af2-fecd-e3041ac66c67/4d487aed-a085-41b4-ba65-f87f8178868d" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_81_51" (IFCTEXT)
    Uniclass2015Title = "Mineral wool fire-stopping" (IFCTEXT)
    Uniclass2015Version = "Products v1.30" (IFCTEXT)
    Version = "16" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCBUILDING)
    Author (no value)
  NBS_Data | properties | on 2 objects (2 IFCCOVERING) | on 3 type objects
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    FirePerformance = "When used in conjunction with CW-FS120 Perimeter Barrier, EI 120. When used in conjunction with CW-FS180 Perimeter Barrier, EI 180" (IFCTEXT)
    Length = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    Recyclability = "Recyclable" (IFCTEXT)
    ThermalConductivity = "0.038 W/m·K" (IFCTEXT)
    ThirdPartyCertification = "Certifire and Intertek certified" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    FirePerformance = "When used in conjunction with CW-FS120 Perimeter Barrier, EI 120. When used in conjunction with CW-FS180 Perimeter Barrier, EI 180" (IFCTEXT)
    Length = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
    Recyclability = "Recyclable" (IFCTEXT)
    ThermalConductivity = "0.038 W/m·K" (IFCTEXT)
    ThirdPartyCertification = "Certifire and Intertek certified" (IFCTEXT)

Other addresses and roles
  2 x postal address: "Enter address here", "Westminster", "London", "UK"