IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2025-05-08T12:07:33"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.70.9 - Exporter 22.4.0.0 - Alternate UI 22.4.0.0"
Application: "Autodesk Revit 2022 (ENG)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENG)"

People and organizations
  Person "Lana.Whittaker" of Organization (no name given)
  Owner history of Person "Lana.Whittaker" of Organization (no name given) | application "Autodesk Revit 2022 (ENG)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENG)" | change NOCHANGE | created 1746701441 (2025-05-08T10:50:41Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:Circle Head - Project Datum" | elevation 0.
        contains 19 elements
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" | object type "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm:221897" | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" | object type "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm:222044" | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" 100.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" | object type "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm:222056" | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" | object type "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm:222068" | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" | object type "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm:222080" | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" 100.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" | object type "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm:222092" | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" | object type "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm:222104" | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" 90.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" | object type "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm:222116" | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" | object type "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm:222128" | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" 150.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" | object type "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" | INSULATION | names: "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm:222589" | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" | object type "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" | INSULATION | names: "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm:222597" | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" 100.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" | object type "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" | INSULATION | names: "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm:222605" | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" | object type "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" | INSULATION | names: "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm:222613" | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" | object type "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" | INSULATION | names: "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm:222621" | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" 100.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" | object type "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" | INSULATION | names: "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm:222629" | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" | object type "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" | INSULATION | names: "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm:222637" | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" 90.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" | object type "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" | INSULATION | names: "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm:222645" | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" | object type "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" | INSULATION | names: "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm:222653" | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" 150.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS180FirestopVoidWidth20–250mm" | object type "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS180FirestopVoidWidth20–250mm" | INSULATION | names: "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS180FirestopVoidWidth20–250mm:222661" | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS180FirestopVoidWidth20–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS180FirestopVoidWidth20–250mm" 150.) | property sets: IFC, COBie, BOS_General, NBS_Data

Types
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" 100.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" 100.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" 90.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" 150.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" 100.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" 100.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" 90.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120XFirestopVoidWidth251–400mm" 150.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS180FirestopVoidWidth20–250mm" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS180FirestopVoidWidth20–250mm" ("NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS180FirestopVoidWidth20–250mm" 150.) | property sets: IFC, COBie, BOS_General, NBS_Data

Property sets
  COBie | properties | on 3 objects (1 IFCBUILDING, 1 IFCPROJECT, 1 IFCSITE)
    Category = "Project Information" (IFCTEXT)
  COBie | properties | on 2 objects (2 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_81_51:Mineral wool fire-stopping" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Firestop and cavity barrier used in curtain walling and sealed facades." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Suitable for horizontal and vertical application, Provides a smoke seal, Quick and simple to install, High fire and acoustic performance" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "CW-FS Firestop and CW-CB Cavity Barrier" (IFCTEXT)
    Name = "MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "60 year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 2 objects (2 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_81_51:Mineral wool fire-stopping" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Firestop and cavity barrier used in curtain walling and sealed facades." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Suitable for horizontal and vertical application, Provides a smoke seal, Quick and simple to install, High fire and acoustic performance" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "CW-FS Firestop and CW-CB Cavity Barrier" (IFCTEXT)
    Name = "MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "60 year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 2 objects (2 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_81_51:Mineral wool fire-stopping" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Firestop and cavity barrier used in curtain walling and sealed facades." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Suitable for horizontal and vertical application, Provides a smoke seal, Quick and simple to install, High fire and acoustic performance" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "CW-FS Firestop and CW-CB Cavity Barrier" (IFCTEXT)
    Name = "MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "60 year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 2 objects (2 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_81_51:Mineral wool fire-stopping" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Firestop and cavity barrier used in curtain walling and sealed facades." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Suitable for horizontal and vertical application, Provides a smoke seal, Quick and simple to install, High fire and acoustic performance" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "CW-FS Firestop and CW-CB Cavity Barrier" (IFCTEXT)
    Name = "MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "60 year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 2 objects (2 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_81_51:Mineral wool fire-stopping" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Firestop and cavity barrier used in curtain walling and sealed facades." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Suitable for horizontal and vertical application, Provides a smoke seal, Quick and simple to install, High fire and acoustic performance" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "CW-FS Firestop and CW-CB Cavity Barrier" (IFCTEXT)
    Name = "MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "60 year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 2 objects (2 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_81_51:Mineral wool fire-stopping" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Firestop and cavity barrier used in curtain walling and sealed facades." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Suitable for horizontal and vertical application, Provides a smoke seal, Quick and simple to install, High fire and acoustic performance" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "CW-FS Firestop and CW-CB Cavity Barrier" (IFCTEXT)
    Name = "MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "60 year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 2 objects (2 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_81_51:Mineral wool fire-stopping" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Firestop and cavity barrier used in curtain walling and sealed facades." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Suitable for horizontal and vertical application, Provides a smoke seal, Quick and simple to install, High fire and acoustic performance" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "CW-FS Firestop and CW-CB Cavity Barrier" (IFCTEXT)
    Name = "MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "60 year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie: 14 more contents on 6 objects not shown
  IFC | properties | on 19 objects (19 IFCCOVERING) | on 19 type objects
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "INSULATION" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth20–50mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    NBSObjectId = "ad56d019-680f-f3d4-7465-031835e0488f" (IFCTEXT)
    NBSVariantId = "fa19dc91-e6bb-74f5-3036-833b7d9a623f" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/ad56d019-680f-f3d4-7465-031835e0488f/5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_81_51" (IFCTEXT)
    Uniclass2015Title = "Mineral wool fire-stopping" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "79" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth20–50mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    NBSObjectId = "ad56d019-680f-f3d4-7465-031835e0488f" (IFCTEXT)
    NBSVariantId = "a26e11a4-01f7-de4e-6d16-349893fc37fd" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/ad56d019-680f-f3d4-7465-031835e0488f/5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_81_51" (IFCTEXT)
    Uniclass2015Title = "Mineral wool fire-stopping" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "79" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth20–50mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    NBSObjectId = "ad56d019-680f-f3d4-7465-031835e0488f" (IFCTEXT)
    NBSVariantId = "ee643e3e-ac18-7b9a-5bca-7366e70d09ec" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/ad56d019-680f-f3d4-7465-031835e0488f/5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_81_51" (IFCTEXT)
    Uniclass2015Title = "Mineral wool fire-stopping" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "79" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30CavityBarrierVoidWidth51–250mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    NBSObjectId = "ad56d019-680f-f3d4-7465-031835e0488f" (IFCTEXT)
    NBSVariantId = "01ca37d5-6e53-bf89-f405-871b3e5ebe87" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/ad56d019-680f-f3d4-7465-031835e0488f/5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_81_51" (IFCTEXT)
    Uniclass2015Title = "Mineral wool fire-stopping" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "79" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60FirestopVoidWidth51–250mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    NBSObjectId = "ad56d019-680f-f3d4-7465-031835e0488f" (IFCTEXT)
    NBSVariantId = "306733f9-13d8-7b7f-b711-576f1ae59891" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/ad56d019-680f-f3d4-7465-031835e0488f/5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_81_51" (IFCTEXT)
    Uniclass2015Title = "Mineral wool fire-stopping" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "79" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS120FirestopVoidWidth51–250mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    NBSObjectId = "ad56d019-680f-f3d4-7465-031835e0488f" (IFCTEXT)
    NBSVariantId = "16bd10d4-1635-43cc-b89d-e4e76daf3eb6" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/ad56d019-680f-f3d4-7465-031835e0488f/5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_81_51" (IFCTEXT)
    Uniclass2015Title = "Mineral wool fire-stopping" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "79" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-CB30XCavityBarrierVoidWidth251–400mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    NBSObjectId = "ad56d019-680f-f3d4-7465-031835e0488f" (IFCTEXT)
    NBSVariantId = "d74d844b-0781-f973-acf6-564ddf15047d" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/ad56d019-680f-f3d4-7465-031835e0488f/5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_81_51" (IFCTEXT)
    Uniclass2015Title = "Mineral wool fire-stopping" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "79" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_MineralWoolFire-stopping_CW-FSFirestopAndCW-CBCavityBarrier_CW-FS60XFirestopVoidWidth251–400mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    NBSObjectId = "ad56d019-680f-f3d4-7465-031835e0488f" (IFCTEXT)
    NBSVariantId = "8af79a2c-126c-743f-14d8-99ddac399499" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/ad56d019-680f-f3d4-7465-031835e0488f/5fe6023e-ba48-44bf-84de-4737bf9045a0" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_81_51" (IFCTEXT)
    Uniclass2015Title = "Mineral wool fire-stopping" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "79" (IFCTEXT)
  BOS_General: 11 more contents on 11 objects not shown
  NBS_Data | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    A1-A3ProductionStage = "1.68" (IFCTEXT)
    Accessories = "Not required,Siderise RFT120/45 tape" (IFCTEXT)
    Compression = "+10%" (IFCTEXT)
    Configuration = "Vertical,Horizontal" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 90 minutes integrity 30 minutes insulation" (IFCTEXT)
    FixingBrackets = "Not required" (IFCTEXT)
    OverallCavityWidth = "To BS EN 1366-4, 20–50 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeLengthxWidth = "1200 mm x (void width)" (IFCTEXT)
    SizeThickness = "75 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 21 (C;Ctr) (-1;-2)" (IFCTEXT)
  NBS_Data | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    A1-A3ProductionStage = "1.68" (IFCTEXT)
    Accessories = "Not required,Siderise RFT120/45 tape" (IFCTEXT)
    Compression = "+10%" (IFCTEXT)
    Configuration = "Vertical,Horizontal" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 90 minutes integrity 60 minutes insulation" (IFCTEXT)
    FixingBrackets = "Not required" (IFCTEXT)
    OverallCavityWidth = "To BS EN 1366-4, 20–50 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeLengthxWidth = "1200 mm x (void width)" (IFCTEXT)
    SizeThickness = "100 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 21 (C;Ctr) (-1;-2)" (IFCTEXT)
  NBS_Data | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    A1-A3ProductionStage = "1.68" (IFCTEXT)
    Accessories = "Not required,Siderise RFT120/45 tape" (IFCTEXT)
    Compression = "+10%" (IFCTEXT)
    Configuration = "Vertical,Horizontal" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 120 minutes integrity 120 minutes insulation.Fire resistance to BS EN 1364-4; 120 minutes integrity 120 minutes insulation" (IFCTEXT)
    FixingBrackets = "Not required,B65/110 - stainless steel (S),B65/110 - galvanized steel (G)" (IFCTEXT)
    OverallCavityWidth = "20–50 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeLengthxWidth = "1200 mm x (void width)" (IFCTEXT)
    SizeThickness = "120 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 23 (C;Ctr) (-1;-3)" (IFCTEXT)
  NBS_Data | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    A1-A3ProductionStage = "1.68" (IFCTEXT)
    Accessories = "Not required,Siderise RFT120/45 tape" (IFCTEXT)
    Compression = "Minimum +10 mm" (IFCTEXT)
    Configuration = "Vertical,Horizontal" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 90 minutes integrity 30 minutes insulation" (IFCTEXT)
    FixingBrackets = "B65/110 - stainless steel (S),B65/110 - galvanized steel (G),B195 - stainless steel (S),B195 - galvanized steel (G)" (IFCTEXT)
    OverallCavityWidth = "To BS EN 1366-4, 51–250 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeLengthxWidth = "1200 mm x (void width)" (IFCTEXT)
    SizeThickness = "75 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 21 (C;Ctr) (-1;-2)" (IFCTEXT)
  NBS_Data | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    A1-A3ProductionStage = "1.68" (IFCTEXT)
    Accessories = "Not required,Siderise RFT120/45 tape" (IFCTEXT)
    Compression = "Minimum +10 mm" (IFCTEXT)
    Configuration = "Vertical,Horizontal" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 90 minutes integrity 60 minutes insulation" (IFCTEXT)
    FixingBrackets = "B65/110 - stainless steel (S),B65/110 - galvanized steel (G),B195 - stainless steel (S),B195 - galvanized steel (G)" (IFCTEXT)
    OverallCavityWidth = "To BS EN 1366-4, 51–250 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeLengthxWidth = "1200 mm x (void width)" (IFCTEXT)
    SizeThickness = "100 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 21 (C;Ctr) (-1;-2)" (IFCTEXT)
  NBS_Data | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    A1-A3ProductionStage = "1.68" (IFCTEXT)
    Accessories = "Not required,Siderise RFT120/45 tape" (IFCTEXT)
    Compression = "To BS EN 1366-4, minimum +10 mm,To BS EN 1364-4, +10%" (IFCTEXT)
    Configuration = "Vertical,Horizontal" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 120 minutes integrity 120 minutes insulation.Fire resistance to BS EN 1364-4; 120 minutes integrity 120 minutes insulation" (IFCTEXT)
    FixingBrackets = "B65/110 - stainless steel (S),B65/110 - galvanized steel (G),B195 - stainless steel (S),B195 - galvanized steel (G)" (IFCTEXT)
    OverallCavityWidth = "51–250 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeLengthxWidth = "1200 mm x (void width)" (IFCTEXT)
    SizeThickness = "120 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 23 (C;Ctr) (-1;-3)" (IFCTEXT)
  NBS_Data | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    A1-A3ProductionStage = "1.68" (IFCTEXT)
    Accessories = "Not required,Siderise RFT120/45 tape" (IFCTEXT)
    Compression = "Minimum +10 mm" (IFCTEXT)
    Configuration = "Vertical,Horizontal" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 90 minutes integrity 30 minutes insulation" (IFCTEXT)
    FixingBrackets = "B355 - stainless steel (S),B355 - galvanized steel (G)" (IFCTEXT)
    OverallCavityWidth = "To BS EN 1366-4, 251–400 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeLengthxWidth = "1200 mm x (void width)" (IFCTEXT)
    SizeThickness = "90 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 21 (C;Ctr) (-1;-2)" (IFCTEXT)
  NBS_Data | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    A1-A3ProductionStage = "1.68" (IFCTEXT)
    Accessories = "Not required,Siderise RFT120/45 tape" (IFCTEXT)
    Compression = "Minimum +10 mm" (IFCTEXT)
    Configuration = "Vertical,Horizontal" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 90 minutes integrity 60 minutes insulation" (IFCTEXT)
    FixingBrackets = "B355 - stainless steel (S),B355 - galvanized steel (G)" (IFCTEXT)
    OverallCavityWidth = "To BS EN 1366-4, 251–400 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeLengthxWidth = "1200 mm x (void width)" (IFCTEXT)
    SizeThickness = "120 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 23 (C;Ctr) (-1;-3)" (IFCTEXT)
  NBS_Data: 2 more contents on 3 objects not shown