IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2017-03-02T14:01:11"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1488463271 (2017-03-02T14:01:11Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1488463271 (2017-03-02T14:01:11Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_SideriseGroup_MnrlWoolFireStpng_NXS" | FLOOR | names: "NBS_SideriseGroup_MnrlWoolFireStpng_NXS" | material: layers "NBS_SideriseGroup_MnrlWoolFireStpng_NXS" ("NBS_SideriseGroup_MnrlWoolFireStpng_NXS" 250.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_SideriseGroup_MnrlWoolFireStpng_NXS" | FLOOR | 1 occurrence | material: layers "NBS_SideriseGroup_MnrlWoolFireStpng_NXS" ("NBS_SideriseGroup_MnrlWoolFireStpng_NXS" 250.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_General, NBS_Data, IFC

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_80_81_51:Mineral wool fire stopping" (IFCTEXT)
    CodePerformance = "BS EN 1364-3: 2006" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Stonewool with silver foil facing one side, net facing opposite side" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Firesafe insulation, Manufactured to bespoke specification" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "sales@siderise.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "SIDERISE NXS Firesafe Spandrel Insulation (formerly Lamatherm NXS)" (IFCTEXT)
    Name = "MineralWoolFireStopping_NXS_SideriseGroup" (IFCTEXT)
    NominalHeight = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "1200 x 1200" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Class A1" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 250. (IFCREAL)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_MnrlWoolFireStpng_NXS" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "www.siderise.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/yoi114pz" (IFCTEXT)
    NBSDescription = "Mineral wool fire stopping" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-45-70/427" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "http://www.siderise.com/applications/products/nxs-firesafe-spandrel-insulation?facades" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_81_51" (IFCTEXT)
    Uniclass2015Title = "Mineral wool fire stopping" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "2" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Fixings = "Bonded" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    ThermalRating = "λ20 = 0.038w/mK" (IFCTEXT)
    ThicknessOptions = "25-250 mm" (IFCTEXT)
    WidthOptions = "Up to 1200 mm" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "INSULATION" (IFCTEXT)