IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2025-02-05T10:23:35"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.70.9 - Exporter 22.4.0.0 - Alternate UI 22.4.0.0"
Application: "Autodesk Revit 2022 (ENG)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENG)"

People and organizations
  Person "erin.hay" of Organization (no name given)
  Owner history of Person "erin.hay" of Organization (no name given) | application "Autodesk Revit 2022 (ENG)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENG)" | change NOCHANGE | created 1738750975 (2025-02-05T10:22:55Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:Circle Head - Project Datum" | elevation 0.
        contains 10 elements
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9030" | object type "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9030" | INSULATION | names: "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9030:221905" | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9030" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9030" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-3030" | object type "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-3030" | INSULATION | names: "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-3030:222060" | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-3030" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-3030" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-6060" | object type "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-6060" | INSULATION | names: "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-6060:222078" | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-6060" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-6060" 90.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9060" | object type "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9060" | INSULATION | names: "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9060:222096" | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9060" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9060" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-12060" | object type "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-12060" | INSULATION | names: "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-12060:222114" | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-12060" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-12060" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-606051–300mmCavities" | object type "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-606051–300mmCavities" | INSULATION | names: "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-606051–300mmCavities:222132" | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-606051–300mmCavities" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-606051–300mmCavities" 90.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-60600–50mmCavities" | object type "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-60600–50mmCavities" | INSULATION | names: "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-60600–50mmCavities:222150" | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-60600–50mmCavities" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-60600–50mmCavities" 35.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-1209026–425mmCavities" | object type "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-1209026–425mmCavities" | INSULATION | names: "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-1209026–425mmCavities:222168" | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-1209026–425mmCavities" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-1209026–425mmCavities" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120900–25mmCavities" | object type "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120900–25mmCavities" | INSULATION | names: "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120900–25mmCavities:222186" | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120900–25mmCavities" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120900–25mmCavities" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120120" | object type "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120120" | INSULATION | names: "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120120:222204" | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120120" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120120" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data

Types
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9030" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9030" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9030" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-3030" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-3030" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-3030" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-6060" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-6060" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-6060" 90.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9060" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9060" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9060" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-12060" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-12060" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-12060" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-606051–300mmCavities" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-606051–300mmCavities" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-606051–300mmCavities" 90.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-60600–50mmCavities" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-60600–50mmCavities" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-60600–50mmCavities" 35.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-1209026–425mmCavities" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-1209026–425mmCavities" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-1209026–425mmCavities" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120900–25mmCavities" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120900–25mmCavities" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120900–25mmCavities" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120120" | INSULATION | 1 occurrence | material: layers "Floor:NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120120" ("NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-120120" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data

Property sets
  COBie | properties | on 3 objects (1 IFCBUILDING, 1 IFCPROJECT, 1 IFCSITE)
    Category = "Project Information" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_44:Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Cavity Fire Barriers for horizontal application in cladding/ rainscreen systems" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Fully compliant to latest ASFP and CWCT guidelines,25 mm or 50mm gap for ventilation and drainage in external cavity" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cavity Barrier, Siderise RH Ventilated Cavity Barrier" (IFCTEXT)
    Name = "IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9030_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_44:Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Cavity Fire Barriers for horizontal application in cladding/ rainscreen systems" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Fully compliant to latest ASFP and CWCT guidelines,25 mm or 50mm gap for ventilation and drainage in external cavity" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cavity Barrier, Siderise RH Ventilated Cavity Barrier" (IFCTEXT)
    Name = "IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-3030_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_44:Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Cavity Fire Barriers for horizontal application in cladding/ rainscreen systems" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Fully compliant to latest ASFP and CWCT guidelines,25 mm or 50mm gap for ventilation and drainage in external cavity" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cavity Barrier, Siderise RH Ventilated Cavity Barrier" (IFCTEXT)
    Name = "IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-6060_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_44:Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Cavity Fire Barriers for horizontal application in cladding/ rainscreen systems" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Fully compliant to latest ASFP and CWCT guidelines,25 mm or 50mm gap for ventilation and drainage in external cavity" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cavity Barrier, Siderise RH Ventilated Cavity Barrier" (IFCTEXT)
    Name = "IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9060_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_44:Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Cavity Fire Barriers for horizontal application in cladding/ rainscreen systems" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Fully compliant to latest ASFP and CWCT guidelines,25 mm or 50mm gap for ventilation and drainage in external cavity" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cavity Barrier, Siderise RH Ventilated Cavity Barrier" (IFCTEXT)
    Name = "IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-12060_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_44:Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Cavity Fire Barriers for horizontal application in cladding/ rainscreen systems" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Fully compliant to latest ASFP and CWCT guidelines,25 mm or 50mm gap for ventilation and drainage in external cavity" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cavity Barrier, Siderise RH Ventilated Cavity Barrier" (IFCTEXT)
    Name = "IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-606051–300mmCavities_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_44:Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Cavity Fire Barriers for horizontal application in cladding/ rainscreen systems" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "Fully compliant to latest ASFP and CWCT guidelines,25 mm or 50mm gap for ventilation and drainage in external cavity" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Cavity Barrier, Siderise RH Ventilated Cavity Barrier" (IFCTEXT)
    Name = "IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-60600–50mmCavities_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle,Other" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie: 14 more contents on 4 objects not shown
  IFC | properties | on 10 objects (10 IFCCOVERING) | on 10 type objects
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "INSULATION" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9030" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    NBSObjectId = "90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659" (IFCTEXT)
    NBSVariantId = "531498c9-1843-0b15-f62c-326f9661950a" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659/187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_44" (IFCTEXT)
    Uniclass2015Title = "Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.36" (IFCTEXT)
    Version = "64" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-3030" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    NBSObjectId = "90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659" (IFCTEXT)
    NBSVariantId = "f63c5f13-de9c-2637-dec2-6128e108978b" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659/187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_44" (IFCTEXT)
    Uniclass2015Title = "Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.36" (IFCTEXT)
    Version = "64" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-6060" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    NBSObjectId = "90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659" (IFCTEXT)
    NBSVariantId = "c428bd1d-b55c-7840-bebf-6415c01ce002" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659/187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_44" (IFCTEXT)
    Uniclass2015Title = "Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.36" (IFCTEXT)
    Version = "64" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-9060" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    NBSObjectId = "90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659" (IFCTEXT)
    NBSVariantId = "bbcf349c-8057-abfb-38be-65a7162b26a6" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659/187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_44" (IFCTEXT)
    Uniclass2015Title = "Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.36" (IFCTEXT)
    Version = "64" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-12060" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    NBSObjectId = "90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659" (IFCTEXT)
    NBSVariantId = "343d2586-e74f-5e10-e34b-5c3b5ab67510" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659/187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_44" (IFCTEXT)
    Uniclass2015Title = "Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.36" (IFCTEXT)
    Version = "64" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-606051–300mmCavities" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    NBSObjectId = "90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659" (IFCTEXT)
    NBSVariantId = "0b5403ec-27d0-86b0-c6f5-ce32a9146aad" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659/187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_44" (IFCTEXT)
    Uniclass2015Title = "Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.36" (IFCTEXT)
    Version = "64" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH50-60600–50mmCavities" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    NBSObjectId = "90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659" (IFCTEXT)
    NBSVariantId = "dac3e7ad-4943-4eb1-d2a9-ff71d3de41bf" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659/187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_44" (IFCTEXT)
    Uniclass2015Title = "Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.36" (IFCTEXT)
    Version = "64" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_IntumescentSleevedMineralWoolCavityFireBarriers_CavityBarrierSideriseRHVentilatedCavityBarrier_RH25-1209026–425mmCavities" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    NBSObjectId = "90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659" (IFCTEXT)
    NBSVariantId = "da02b163-e41e-e5bc-9e78-3a973318b209" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/90c6ad8f-ffe8-b6e0-b6bc-9fc85c391659/187e0dfb-d331-4e25-95ff-16d70a4acdec" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_44" (IFCTEXT)
    Uniclass2015Title = "Intumescent sleeved mineral wool cavity fire barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.36" (IFCTEXT)
    Version = "64" (IFCTEXT)
  BOS_General: 2 more contents on 2 objects not shown
  NBS_Data | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    AirGap = "≤25 mm" (IFCTEXT)
    Attachment = "See Fixing method" (IFCTEXT)
    CavityWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Colour = "Identifying strip colour - green" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    EmbodiedCarbon = "1.85" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "To EN 13501-1, Class A1 (primary stonewool seal).To EN 13501-1, Class E (intumescent strip only)" (IFCTEXT)
    FireResistance = "To ASFP TGD19, integrity E 90; insulation I 30" (IFCTEXT)
    FixingMethod = "n/a" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    Standard = "Tested in accordance with ASFP Technical Guidance Document TDG19" (IFCTEXT)
    ThermalConductivity = "0.038 W/m·K" (IFCTEXT)
    Thickness = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    Third-partyCertification = "IFC Certification IFCC 1712" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    AirGap = "≤50 mm" (IFCTEXT)
    Attachment = "See Fixing method" (IFCTEXT)
    CavityWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Colour = "Identifying strip colour - red" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    EmbodiedCarbon = "1.85" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "To EN 13501-1, Class A1 (primary stonewool seal).To EN 13501-1, Class E (intumescent strip only)" (IFCTEXT)
    FireResistance = "To ASFP TGD19, integrity E 30; insulation I 30" (IFCTEXT)
    FixingMethod = "n/a" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    Standard = "Tested in accordance with ASFP Technical Guidance Document TDG19" (IFCTEXT)
    ThermalConductivity = "0.038 W/m·K" (IFCTEXT)
    Thickness = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    Third-partyCertification = "IFC Certification IFCC 1712" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    AirGap = "≤25 mm" (IFCTEXT)
    Attachment = "See Fixing method" (IFCTEXT)
    CavityWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Colour = "Identifying strip colour - orange" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    EmbodiedCarbon = "1.85" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "To EN 13501-1, Class A1 (primary stonewool seal).To EN 13501-1, Class E (intumescent strip only)" (IFCTEXT)
    FireResistance = "To ASFP TGD19, integrity E 60; insulation I 60" (IFCTEXT)
    FixingMethod = "n/a" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    Standard = "Tested in accordance with ASFP Technical Guidance Document TDG19" (IFCTEXT)
    ThermalConductivity = "0.038 W/m·K" (IFCTEXT)
    Thickness = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Third-partyCertification = "IFC Certification IFCC 1712" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    AirGap = "≤25 mm" (IFCTEXT)
    Attachment = "See Fixing method" (IFCTEXT)
    CavityWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Colour = "Identifying strip colour - purple" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    EmbodiedCarbon = "1.85" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "To EN 13501-1, Class A1 (primary stonewool seal).To EN 13501-1, Class E (intumescent strip only)" (IFCTEXT)
    FireResistance = "To ASFP TGD19, integrity E 90; insulation I 60" (IFCTEXT)
    FixingMethod = "n/a" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    Standard = "Tested in accordance with ASFP Technical Guidance Document TDG19" (IFCTEXT)
    ThermalConductivity = "0.038 W/m·K" (IFCTEXT)
    Thickness = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    Third-partyCertification = "IFC Certification IFCC 1712" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    AirGap = "≤25 mm" (IFCTEXT)
    Attachment = "See Fixing method" (IFCTEXT)
    CavityWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Colour = "Identifying strip colour - yellow" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    EmbodiedCarbon = "1.85" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "To EN 13501-1, Class A1 (primary stonewool seal).To EN 13501-1, Class E (intumescent strip only)" (IFCTEXT)
    FireResistance = "To ASFP TGD19, integrity E 120; insulation I 60" (IFCTEXT)
    FixingMethod = "n/a" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    Standard = "Tested in accordance with ASFP Technical Guidance Document TDG19" (IFCTEXT)
    ThermalConductivity = "0.038 W/m·K" (IFCTEXT)
    Thickness = 120. (IFCLENGTHMEASURE) [MILLI METRE]
    Third-partyCertification = "IFC Certification IFCC 1712" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    AirGap = "≤50 mm" (IFCTEXT)
    Attachment = "See Fixing method" (IFCTEXT)
    CavityWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Colour = "Identifying strip colour - blue" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    EmbodiedCarbon = "1.85" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "To EN 13501-1, Class A1 (primary stonewool seal).To EN 13501-1, Class E (intumescent strip only)" (IFCTEXT)
    FireResistance = "To ASFP TGD19, integrity E 60; insulation I 60" (IFCTEXT)
    FixingMethod = "n/a" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    Standard = "Tested in accordance with ASFP Technical Guidance Document TDG19" (IFCTEXT)
    ThermalConductivity = "0.038 W/m·K" (IFCTEXT)
    Thickness = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Third-partyCertification = "IFC Certification IFCC 1712" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    AirGap = "≤50 mm" (IFCTEXT)
    Attachment = "See Fixing method" (IFCTEXT)
    CavityWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Colour = "Intumescent strip only - blue" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    EmbodiedCarbon = "1.85" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "To EN 13501-1, Class A1 (primary stonewool seal).To EN 13501-1, Class E (intumescent strip only)" (IFCTEXT)
    FireResistance = "To ASFP TGD19, integrity E 60; insulation I 60" (IFCTEXT)
    FixingMethod = "Secured to substrate with screw fixings, installed at 400 mm centres based on a 1200 mm strip.For lengths ≤800 mm 2no screw fixings must be used, with spacing reduced pro-rata.Lengths • All barriers to be suitably fixed to substrate with non-combustible fixings and washers with a 15 mm (maximum) head diameter" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    Standard = "Tested in accordance with ASFP Technical Guidance Document TDG19" (IFCTEXT)
    ThermalConductivity = "0.038 W/m·K" (IFCTEXT)
    Thickness = 35. (IFCLENGTHMEASURE) [MILLI METRE]
    Third-partyCertification = "IFC Certification IFCC 1712" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    AirGap = "≤25 mm" (IFCTEXT)
    Attachment = "See Fixing method" (IFCTEXT)
    CavityWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Colour = "Identifying strip colour - grey" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    EmbodiedCarbon = "1.85" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "To EN 13501-1, Class A1 (primary stonewool seal).To EN 13501-1, Class E (intumescent strip only)" (IFCTEXT)
    FireResistance = "To ASFP TGD19, integrity E 120; insulation I 90" (IFCTEXT)
    FixingMethod = "n/a" (IFCTEXT)
    Material = "Stonewool,Aluminium,Intumescent,Stone wool,Rock fibre mineral wool,Fibre,Foil,Mineral wool,Mineral fibre,Mineral" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    Standard = "Tested in accordance with ASFP Technical Guidance Document TDG19" (IFCTEXT)
    ThermalConductivity = "0.038 W/m·K" (IFCTEXT)
    Thickness = 120. (IFCLENGTHMEASURE) [MILLI METRE]
    Third-partyCertification = "IFC Certification IFCC 1712" (IFCTEXT)
  NBS_Data: 2 more contents on 2 objects not shown