IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement []"
File name: "Project Number"
Time stamp: "2025-04-28T11:42:17"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.70.9 - Exporter 22.4.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENG)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENG)"

People and organizations
  Person "Lana.Whittaker" of Organization (no name given)
  Owner history of Person "Lana.Whittaker" of Organization (no name given) | application "Autodesk Revit 2022 (ENG)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENG)" | change NOCHANGE | created 1745836934 (2025-04-28T10:42:14Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  SOUNDPOWERUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:Circle Head - Project Datum" | elevation 0.
        contains 19 elements
          1 x IFCANNOTATION | object type "Text:10 mm Arial" | names: "Text:10 mm Arial:212700" | property sets: COBie, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth20–50mm" | object type "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth20–50mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth20–50mm:221903" | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth20–50mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth20–50mm" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
          9 x IFCANNOTATION | object type "Text:2.5mm Arial" | names: "Text:2.5mm Arial:222051", "Text:2.5mm Arial:222063", "Text:2.5mm Arial:222075" (+6 more) | property sets: COBie, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth20–50mm" | object type "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth20–50mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth20–50mm:222056" | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth20–50mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth20–50mm" 100.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth20–50mm" | object type "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth20–50mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth20–50mm:222068" | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth20–50mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth20–50mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth51–250mm" | object type "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth51–250mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth51–250mm:222080" | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth51–250mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth51–250mm" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth51–250mm" | object type "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth51–250mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth51–250mm:222092" | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth51–250mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth51–250mm" 100.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth51–250mm" | object type "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth51–250mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth51–250mm:222104" | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth51–250mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth51–250mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030XCavityBarrierVoidWidth251–400mm" | object type "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030XCavityBarrierVoidWidth251–400mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030XCavityBarrierVoidWidth251–400mm:222116" | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030XCavityBarrierVoidWidth251–400mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030XCavityBarrierVoidWidth251–400mm" 90.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060XCavityBarrierVoidWidth251–400mm" | object type "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060XCavityBarrierVoidWidth251–400mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060XCavityBarrierVoidWidth251–400mm:222128" | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060XCavityBarrierVoidWidth251–400mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060XCavityBarrierVoidWidth251–400mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120XCavityBarrierVoidWidth251–400mm" | object type "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120XCavityBarrierVoidWidth251–400mm" | INSULATION | names: "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120XCavityBarrierVoidWidth251–400mm:222140" | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120XCavityBarrierVoidWidth251–400mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120XCavityBarrierVoidWidth251–400mm" 150.) | property sets: IFC, COBie, BOS_General, NBS_Data

Types
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth20–50mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth20–50mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth20–50mm" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth20–50mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth20–50mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth20–50mm" 100.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth20–50mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth20–50mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth20–50mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth51–250mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth51–250mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth51–250mm" 75.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth51–250mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth51–250mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth51–250mm" 100.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth51–250mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth51–250mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth51–250mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030XCavityBarrierVoidWidth251–400mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030XCavityBarrierVoidWidth251–400mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030XCavityBarrierVoidWidth251–400mm" 90.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060XCavityBarrierVoidWidth251–400mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060XCavityBarrierVoidWidth251–400mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060XCavityBarrierVoidWidth251–400mm" 120.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120XCavityBarrierVoidWidth251–400mm" | INSULATION | 1 occurrence | material: layers "Basic Wall:NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120XCavityBarrierVoidWidth251–400mm" ("NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120XCavityBarrierVoidWidth251–400mm" 150.) | property sets: IFC, COBie, BOS_General, NBS_Data

Property sets
  COBie | properties | on 10 objects (10 IFCANNOTATION)
    Category = "Text Notes" (IFCTEXT)
  COBie | properties | on 3 objects (1 IFCBUILDING, 1 IFCPROJECT, 1 IFCSITE)
    Category = "Project Information" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_79:Sleeved mineral wool cavity barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Siderise RV vertical cavity barriers for rainscreen cladding are used to full fill the void between the external envelope and internal substrate." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Siderise RV Vertical Cavity Barrier" (IFCTEXT)
    Name = "SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth20–50mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "1200 mm x (void width)" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_79:Sleeved mineral wool cavity barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Siderise RV vertical cavity barriers for rainscreen cladding are used to full fill the void between the external envelope and internal substrate." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Siderise RV Vertical Cavity Barrier" (IFCTEXT)
    Name = "SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth20–50mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "1200 mm x (void width)" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_79:Sleeved mineral wool cavity barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Siderise RV vertical cavity barriers for rainscreen cladding are used to full fill the void between the external envelope and internal substrate." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Siderise RV Vertical Cavity Barrier" (IFCTEXT)
    Name = "SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth20–50mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "1200 mm x (void width)" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_79:Sleeved mineral wool cavity barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Siderise RV vertical cavity barriers for rainscreen cladding are used to full fill the void between the external envelope and internal substrate." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Siderise RV Vertical Cavity Barrier" (IFCTEXT)
    Name = "SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth51–250mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "1200 mm x (void width)" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_79:Sleeved mineral wool cavity barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Siderise RV vertical cavity barriers for rainscreen cladding are used to full fill the void between the external envelope and internal substrate." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Siderise RV Vertical Cavity Barrier" (IFCTEXT)
    Name = "SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth51–250mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "1200 mm x (void width)" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_80_80_79:Sleeved mineral wool cavity barriers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Siderise RV vertical cavity barriers for rainscreen cladding are used to full fill the void between the external envelope and internal substrate." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Foil" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "projects@siderise.com" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Siderise RV Vertical Cavity Barrier" (IFCTEXT)
    Name = "SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth51–250mm_SideriseGroup" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "1200 mm x (void width)" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie: 13 more contents on 4 objects not shown
  NBS_Data | properties | on 9 objects (9 IFCANNOTATION)
    Type = "2.5mm Arial" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCANNOTATION)
    Type = "10 mm Arial" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING)
    A1-A3ProductionStage = "1.72" (IFCTEXT)
    Accessories = "Siderise RFT120/45 Tape" (IFCTEXT)
    CavityBarriersSleeves = "Aluminium foil to surfaces exposed to cavity" (IFCTEXT)
    Compression = "Minimum +10%" (IFCTEXT)
    Configuration = "Vertical" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 90 minutes integrity, 30 minutes insulation" (IFCTEXT)
    FixingBrackets = "Not required" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    NominalDensity = "75 kg/m³" (IFCTEXT)
    OverallCavityWidth = "20–50 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeThickness = "75 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    Third-partyCertification = "IFCC 1712 (BS EN 1366-4).Intertek UK WHI-09-02-22-000001(BS EN 13501-1).Intertek US WHI20-32944302 (BS EN 13501-1)" (IFCTEXT)
    Type = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth20–50mm" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 21 (C;Ctr) (-1;-2)" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING)
    A1-A3ProductionStage = "1.72" (IFCTEXT)
    Accessories = "Siderise RFT120/45 Tape" (IFCTEXT)
    CavityBarriersSleeves = "Aluminium foil to surfaces exposed to cavity" (IFCTEXT)
    Compression = "Minimum +10%" (IFCTEXT)
    Configuration = "Vertical" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 90 minutes integrity, 60 minutes insulation" (IFCTEXT)
    FixingBrackets = "Not required" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    NominalDensity = "75 kg/m³" (IFCTEXT)
    OverallCavityWidth = "20–50 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeThickness = "100 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    Third-partyCertification = "IFCC 1712 (BS EN 1366-4).Intertek UK WHI-09-02-22-000001(BS EN 13501-1).Intertek US WHI20-32944302 (BS EN 13501-1)" (IFCTEXT)
    Type = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth20–50mm" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 21 (C;Ctr) (-1;-2)" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING)
    A1-A3ProductionStage = "1.72" (IFCTEXT)
    Accessories = "Siderise RFT120/45 Tape" (IFCTEXT)
    CavityBarriersSleeves = "Aluminium foil to surfaces exposed to cavity" (IFCTEXT)
    Compression = "Minimum +10%" (IFCTEXT)
    Configuration = "Vertical" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 120 minutes integrity, 120 minutes insulation" (IFCTEXT)
    FixingBrackets = "Not required" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    NominalDensity = "75 kg/m³" (IFCTEXT)
    OverallCavityWidth = "20–50 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeThickness = "120 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    Third-partyCertification = "IFCC 1712 (BS EN 1366-4).Intertek UK WHI-09-02-22-000001(BS EN 13501-1).Intertek US WHI20-32944302 (BS EN 13501-1)" (IFCTEXT)
    Type = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth20–50mm" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 23 (C;Ctr) (-1;-3)" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING)
    A1-A3ProductionStage = "1.72" (IFCTEXT)
    Accessories = "Siderise RFT120/45 Tape" (IFCTEXT)
    CavityBarriersSleeves = "Aluminium foil to surfaces exposed to cavity" (IFCTEXT)
    Compression = "Minimum +10 mm" (IFCTEXT)
    Configuration = "Vertical" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 90 minutes integrity, 30 minutes insulation" (IFCTEXT)
    FixingBrackets = "B65/110 - stainless steel (S),B65/110 - galvanized steel (G),B195 - stainless steel (S),B195 - galvanized steel (G)" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    NominalDensity = "75 kg/m³" (IFCTEXT)
    OverallCavityWidth = "51–250 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeThickness = "75 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    Third-partyCertification = "IFCC 1712 (BS EN 1366-4).Intertek UK WHI-09-02-22-000001(BS EN 13501-1).Intertek US WHI20-32944302 (BS EN 13501-1)" (IFCTEXT)
    Type = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth51–250mm" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 21 (C;Ctr) (-1;-2)" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING)
    A1-A3ProductionStage = "1.72" (IFCTEXT)
    Accessories = "Siderise RFT120/45 Tape" (IFCTEXT)
    CavityBarriersSleeves = "Aluminium foil to surfaces exposed to cavity" (IFCTEXT)
    Compression = "Minimum +10 mm" (IFCTEXT)
    Configuration = "Vertical" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 90 minutes integrity, 60 minutes insulation" (IFCTEXT)
    FixingBrackets = "B65/110 - stainless steel (S),B65/110 - galvanized steel (G),B195 - stainless steel (S),B195 - galvanized steel (G)" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    NominalDensity = "75 kg/m³" (IFCTEXT)
    OverallCavityWidth = "51–250 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeThickness = "100 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    Third-partyCertification = "IFCC 1712 (BS EN 1366-4).Intertek UK WHI-09-02-22-000001(BS EN 13501-1).Intertek US WHI20-32944302 (BS EN 13501-1)" (IFCTEXT)
    Type = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth51–250mm" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 21 (C;Ctr) (-1;-2)" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING)
    A1-A3ProductionStage = "1.72" (IFCTEXT)
    Accessories = "Siderise RFT120/45 Tape" (IFCTEXT)
    CavityBarriersSleeves = "Aluminium foil to surfaces exposed to cavity" (IFCTEXT)
    Compression = "Minimum +10 mm" (IFCTEXT)
    Configuration = "Vertical" (IFCTEXT)
    ContainsRedListMaterials = "No" (IFCTEXT)
    CountryOfMaterialOrigin = "United Kingdom" (IFCTEXT)
    CountryOfProductManufacture = "United Kingdom" (IFCTEXT)
    ExpectedLife = "60 year" (IFCTEXT)
    FirePerformance = "Reaction to fire to EN 13501-1; Class A1.Fire resistance to BS EN 1366-4; 120 minutes integrity, 120 minutes insulation" (IFCTEXT)
    FixingBrackets = "B65/110 - stainless steel (S),B65/110 - galvanized steel (G),B195 - stainless steel (S),B195 - galvanized steel (G)" (IFCTEXT)
    Material = "Stonewool" (IFCTEXT)
    NominalDensity = "75 kg/m³" (IFCTEXT)
    OverallCavityWidth = "51–250 mm" (IFCTEXT)
    Recyclability = "Recyclable" (IFCTEXT)
    SizeThickness = "120 mm" (IFCTEXT)
    ThermalConductivity = "To EN 12667, 0.038 W/m·K" (IFCTEXT)
    Third-partyCertification = "IFCC 1712 (BS EN 1366-4).Intertek UK WHI-09-02-22-000001(BS EN 13501-1).Intertek US WHI20-32944302 (BS EN 13501-1)" (IFCTEXT)
    Type = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth51–250mm" (IFCTEXT)
    WeightedSoundReductionIndexRw = "Rw 23 (C;Ctr) (-1;-3)" (IFCTEXT)
  NBS_Data: 13 more contents on 4 objects not shown
  IFC | properties | on 9 objects (9 IFCCOVERING) | on 9 type objects
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "INSULATION" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth20–50mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    NBSObjectId = "fab0dcbf-4396-4015-ad37-b6740915436c" (IFCTEXT)
    NBSVariantId = "fa0987b6-64df-2be2-02cf-504d37f966b5" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/fab0dcbf-4396-4015-ad37-b6740915436c/3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_79" (IFCTEXT)
    Uniclass2015Title = "Sleeved mineral wool cavity barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "39" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth20–50mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    NBSObjectId = "fab0dcbf-4396-4015-ad37-b6740915436c" (IFCTEXT)
    NBSVariantId = "8a38cdba-3a80-8686-fe99-97be377aa0ce" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/fab0dcbf-4396-4015-ad37-b6740915436c/3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_79" (IFCTEXT)
    Uniclass2015Title = "Sleeved mineral wool cavity barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "39" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth20–50mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    NBSObjectId = "fab0dcbf-4396-4015-ad37-b6740915436c" (IFCTEXT)
    NBSVariantId = "7fcbd822-8efa-1c3b-488d-3a7a6b36cc3c" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/fab0dcbf-4396-4015-ad37-b6740915436c/3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_79" (IFCTEXT)
    Uniclass2015Title = "Sleeved mineral wool cavity barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "39" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030CavityBarrierVoidWidth51–250mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    NBSObjectId = "fab0dcbf-4396-4015-ad37-b6740915436c" (IFCTEXT)
    NBSVariantId = "c005e77e-635d-223f-bc20-6e0c96656a20" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/fab0dcbf-4396-4015-ad37-b6740915436c/3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_79" (IFCTEXT)
    Uniclass2015Title = "Sleeved mineral wool cavity barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "39" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060CavityBarrierVoidWidth51–250mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    NBSObjectId = "fab0dcbf-4396-4015-ad37-b6740915436c" (IFCTEXT)
    NBSVariantId = "0426c121-9648-be2a-2ae5-cf7986a564a6" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/fab0dcbf-4396-4015-ad37-b6740915436c/3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_79" (IFCTEXT)
    Uniclass2015Title = "Sleeved mineral wool cavity barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "39" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-120120CavityBarrierVoidWidth51–250mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    NBSObjectId = "fab0dcbf-4396-4015-ad37-b6740915436c" (IFCTEXT)
    NBSVariantId = "645f1462-e23e-70d1-1920-9958de8d361e" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/fab0dcbf-4396-4015-ad37-b6740915436c/3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_79" (IFCTEXT)
    Uniclass2015Title = "Sleeved mineral wool cavity barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "39" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9030XCavityBarrierVoidWidth251–400mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    NBSObjectId = "fab0dcbf-4396-4015-ad37-b6740915436c" (IFCTEXT)
    NBSVariantId = "68213082-2f3d-1ddc-c0c8-a5f8e6b265bd" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/fab0dcbf-4396-4015-ad37-b6740915436c/3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_79" (IFCTEXT)
    Uniclass2015Title = "Sleeved mineral wool cavity barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "39" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_SideriseGroup_SleevedMineralWoolCavityBarriers_SideriseRVVerticalCavityBarrier_RV-9060XCavityBarrierVoidWidth251–400mm" (IFCTEXT)
    ManufacturerName = "Siderise Group" (IFCTEXT)
    ManufacturerURL = "https://www.siderise.com/" (IFCTEXT)
    NBSInstanceId = "3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    NBSObjectId = "fab0dcbf-4396-4015-ad37-b6740915436c" (IFCTEXT)
    NBSVariantId = "e2b0d56e-c487-82bb-05a0-74185bc0f11a" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/fab0dcbf-4396-4015-ad37-b6740915436c/3b0113fd-1a11-4d4a-9003-8e550884dd84" (IFCTEXT)
    Uniclass2015Code = "Pr_25_80_80_79" (IFCTEXT)
    Uniclass2015Title = "Sleeved mineral wool cavity barriers" (IFCTEXT)
    Uniclass2015Version = "Products v1.37" (IFCTEXT)
    Version = "39" (IFCTEXT)
  BOS_General: 1 more content on 1 objects not shown